Interoperability Priority Items:

Definition: The ability of registered MSI providers to use a single interface, common data formats and architecture to disseminate their MSI via multiple recognised mobile satellite service providers in accordance with the requirements of the IMO.

Methods used – email, smtp, pstn, x25, web interface, machine-to-machine (APIs),

1. Ability to format a message in accordance to the message elements table with the Joint Manual;
2. Ability to create a message once for multiple use by all mobile satellite service providers without additional interaction by the message drafter;